|  |
| --- |
| IVI‑6.2: VISA Interoperability Requirements for USBTMC Specification  November 1, 2018 Edition Revision 1.0 |

Important Information

IVI-6.2: VISA Interoperability Requirements for USBTMC Specification is authored by the IVI Foundation member companies. For a vendor membership roster list, please visit the IVI Foundation web site at www.ivifoundation.org.

The IVI Foundation wants to receive your comments on this specification. You can contact the Foundation through the web site at www.ivifoundation.org.

Warranty

The IVI Foundation and its member companies make no warranty of any kind with regard to this material, including, but not limited to, the implied warranties of merchantability and fitness for a particular purpose. The IVI Foundation and its member companies shall not be liable for errors contained herein or for incidental or consequential damages in connection with the furnishing, performance, or use of this material.

Trademarks

Product and company names listed are trademarks or trade names of their respective companies.

No investigation has been made of common‑law trademark rights in any work.

|  |  |
| --- | --- |
|  |  |

[Important Information 2](#_Toc525115865)

[Warranty 2](#_Toc525115866)

[Trademarks 2](#_Toc525115867)

[IVI‑6.2 VISA Interoperability Requirements for USBTMC 5](#_Toc525115868)

[1. Overview of the VISA Interoperability Requirements for USBTMC Specification 6](#_Toc525115869)

[1.1 Introduction 6](#_Toc525115870)

[1.2 Audience of Specification 6](#_Toc525115871)

[1.3 Organization of Specification 6](#_Toc525115872)

[1.4 VISA Interoperability Requirements for USBTMC Overview 6](#_Toc525115873)

[1.5 References 6](#_Toc525115874)

[1.6 Definition of Terms and Acronyms 7](#_Toc525115875)

[2. Windows Specific Information 9](#_Toc525115876)

[2.1 CreateFile() 9](#_Toc525115877)

[2.2 WriteFile() 9](#_Toc525115878)

[2.3 ReadFile() 10](#_Toc525115879)

[2.4 DeviceIoControl() 10](#_Toc525115880)

[2.4.1 IOCTL\_USBTMC\_GETINFO 11](#_Toc525115881)

[2.4.1.1 Data structure – USBTMC\_DRV\_INFO 12](#_Toc525115882)

[2.4.2 IOCTL\_USBTMC\_CANCEL\_IO 12](#_Toc525115883)

[2.4.2.1 Data Structures – USBTMC\_PIPE\_TYPE 13](#_Toc525115884)

[2.4.3 IOCTL\_USBTMC\_WAIT\_INTERRUPT 14](#_Toc525115885)

[2.4.4 IOCTL\_USBTMC\_RESET\_PIPE 15](#_Toc525115886)

[2.4.5 IOCTL\_USBTMC\_SEND\_REQUEST 15](#_Toc525115887)

[2.4.5.1 Data Structure – USBTMC\_IO\_BLOCK 16](#_Toc525115888)

[2.4.6 IOCTL\_USBTMC\_GET\_LAST\_ERROR 17](#_Toc525115889)

[2.5 CloseHandle() 17](#_Toc525115890)

[2.6 INF files for USBTMC devices 17](#_Toc525115891)

[2.6.1 Class and ClassGUID for USBTMC devices 18](#_Toc525115892)

[2.6.2 INF ClassInstall32 section 18](#_Toc525115893)

[2.6.3 INF DDInstall.Interfaces section 18](#_Toc525115894)

[2.6.4 Product specific INF files 18](#_Toc525115895)

[2.6.5 Class, SubClass, Protocol specific INF files 19](#_Toc525115896)

[2.6.6 Class, SubClass specific INF files and Class specific INF files 19](#_Toc525115897)

[3. USBTMC include file 21](#_Toc525115898)

[4. Available USBD Functions 23](#_Toc525115899)

[Appendix A Linux Specific Information 27](#_Toc525115900)

[A.1 History 27](#_Toc525115901)

[A.2 Added Features 27](#_Toc525115902)

[A.2.1 Changes to Ioctl USBTMC-USB488 READ\_STB 27](#_Toc525115903)

[A.2.2 Support for receiving SRQ notifications via poll/select 27](#_Toc525115904)

[A.2.3 New for IVI: ioctl USBTMC488\_IOCTL\_WAIT\_SRQ 28](#_Toc525115905)

[A.2.4 New ioctl USBTMC488\_IOCTL\_TRIGGER 28](#_Toc525115906)

[A.2.5 New ioctls USBTMC\_IOCTL\_GET/SET\_TIMEOUT 28](#_Toc525115907)

[A.2.6 New ioctl USBTMC\_IOCTL\_CTRL\_REQUEST 28](#_Toc525115908)

[A.2.7 New ioctl USBTMC\_IOCTL\_EOM\_ENABLE 29](#_Toc525115909)

[A.2.8 New ioctl USBTMC\_IOCTL\_CONFIG\_TERMCHAR 29](#_Toc525115910)

[A.2.9 New ioctl USBTMC\_IOCTL\_MSG\_IN\_ATTR 29](#_Toc525115911)

[A.2.10 New ioctl USBTMC\_IOCTL\_WRITE 29](#_Toc525115912)

[A.2.11 New ioctl USBTMC\_IOCTL\_WRITE\_RESULT 30](#_Toc525115913)

[A.2.12 New ioctl USBTMC\_IOCTL\_READ 30](#_Toc525115914)

[A.2.13 New ioctl USBTMC\_IOCTL\_CANCEL\_IO 31](#_Toc525115915)

[A.2.14 New ioctl USBTMC\_IOCTL\_CLEANUP\_IO 31](#_Toc525115916)

[A.2.15 New ioctl USBTMC\_IOCTL\_AUTO\_ABORT 31](#_Toc525115917)

[A.2.16 New ioctl USBTMC\_IOCTL\_API\_VERSION 31](#_Toc525115918)

[A.3 Test Functions 31](#_Toc525115919)

[A.3.1 USBTMC\_IOCTL\_SET\_OUT\_HALT 31](#_Toc525115920)

[A.3.2 USBTMC\_IOCTL\_SET\_IN\_HALT 32](#_Toc525115921)

[A.3.3 USBTMC\_IOCTL\_ABORT\_BULK\_IN\_TAG 32](#_Toc525115922)

[A.3.4 USBTMC\_IOCTL\_ABORT\_BULK\_OUT\_TAG 32](#_Toc525115923)

IVI‑6.2 VISA Interoperability Requirements for USBTMC

VISA Interoperability Requirements for USBTMC Revision History

This section is an overview of the revision history of the VISA Interoperability Requirements for USBTMC specification.

| **Table 1‑1.** VISA Interoperability Requirements for USBTMC Specification Revisions | | |
| --- | --- | --- |
| Revision Number | Date of Revision | Revision Notes |
| Revision 1.0 | March 23, 2010 | First approved version. |
| Revision 1.0 | November 1, 2018 | Editorial change to add the informational appendix describing the Linux USBTMC kernel driver. |

# Overview of the VISA Interoperability Requirements for USBTMC Specification

## Introduction

This section summarizes the VISA Interoperability Requirements for USBTMC Specification itself and contains general information that the reader may need to understand, interpret, and implement aspects of this specification. These aspects include the following:

* Audience
* Organization
* Overview
* References
* Terms and Acronyms

## Audience of Specification

The intended readers for this specification are the vendors who wish to interface with the IVI Foundation USBTMC Windows operating systems drivers, and the implementors of the IVI Foundation USBTMC Windows operating systems drivers.

## Organization of Specification

This specification is organized in sections, with each section discussing a particular aspect of the VISA model. Section 3, *Windows Specific Information*, describes the USBTMC Windows operating systems drivers. Section 4, *USBTMC Include File*, presents the USBTMC driver include file. Section 5, *Available USBTMC Functions*, lists the available USBTMC functions.

## VISA Interoperability Requirements for USBTMC Overview

To achieve USBTMC interoperability, a VISA I/O library running in user-space must be able to interact with the USB Host kernel driver stack in a predictable way. The accepted strategy is to specify the kernel API – the system call semantics and behaviors. This enables a VISA I/O library to communicate successfully with the IVI USBTMC kernel driver.

For Windows, specifying an API means specifying the behaviors of CreateFile (), WriteFile (), ReadFile (), DeviceIoControl (), and CloseHandle ().

In addition to the specification of an API, error codes must be specified. This is because a VISA I/O library implementing the USBTMC specification or a USBTMC subclass specification must know when certain error conditions occur.

## References

Several other documents and specifications are related to this specification. These other related documents are the following:

**USB Implementers Forum**

* USB 2.0 Specification (www.usb.org)
* USBTMC Specification (<http://www.usb.org/developers/devclass_docs#approved>)
* USBTMC USB488 Specification (<http://www.usb.org/developers/devclass_docs#approved>)

**Microsoft**

* Microsoft Platform SDKs for Windows operating systems
* Microsoft DDKs for Windows operating systems

**IVI Foundation** ([www.ivifoundation.org](http://www.ivifoundation.org))

* VPP-4.3 & 4.3.x, The VISA Library and detailed VISA and VISA-COM specifications
* VPP‑9: Instrument Vendor Abbreviations

## Definition of Terms and Acronyms

The following are some commonly used terms and acronyms used in this document.

|  |  |
| --- | --- |
|  |  |
| **API** | Application Programmers Interface. The direct interface that an end user sees when creating an application. The VISA API consists of the sum of all of the operations, attributes, and events of each of the VISA Resource Classes. |
| **Host** | This is similar to the term “Controller” used in other VISA specifications. From the USB 2.0 specification: “The host computer system where the Host Controller is installed. This includes the host software platform (CPU, bus, etc.) and the operating system in use.” |
| **Instrument Driver** | Library of functions for controlling a specific instrument |
| **IRP** | I/O Request Packet. From the USB 2.0 specification: “An identifiable request by a software client to move data between itself (on the host) and an endpoint of a device in an appropriate direction.” |
| **SRQ** | IEEE 488 Service Request. This is an asynchronous request from a remote GPIB device that requires service. A service request is essentially an interrupt from a remote device. For USBTMC, this is a notification on the interrupt IN pipe. |
| **USBTMC client software** | USBTMC software resident on the host that interacts with the USB System Software to arrange data transfer between a function and the host. The client is often the data provider and consumer for transferred data. A VISA I/O library implementation for USBTMC is the USBTMC client software. |
| **USBTMC device dependent command message** | A type of USBTMC command message in which the USBTMC message data bytes are a sequence of bytes defined by the device vendor. Typically a query for a measurement result or a request to change measurement state. Sent from a Host to a device. The VISA method viWrite transfers these messages. |
| **USBTMC interface** | A collection of endpoints on a device that conform to the requirements in this USB Test and Measurement Class specification and can be used to provide the physical/signaling/packet connectivity to a Host. The interface descriptor must have bInterfaceClass and bInterfaceSubClass equal to the appropriate values for a USB Test and Measurement Class interface. |
| **USBTMC response message** | A type of USBTMC message containing a response to a USBTMC command message. Sent from a device to a Host. The VISA method viRead transfers these messages. |

# Windows Specific Information

The Windows system call behaviors for a USBTMC driver are defined here to resemble the behaviors for a pass-through driver. A pass-through driver allows software to send bulk-OUT and control pipe requests with arbitrary content and to receive bulk-IN and interrupt-IN packets with arbitrary content. The motivation to define system call behaviors in this way are:

* Minimizes the work done by the kernel driver.
* Enables the USBTMC protocol and USBTMC subclass protocols to be implemented in user-space, which is easier to debug and is less likely to crash the system.
* Makes it easy to change the protocol above the kernel driver. The kernel driver does not need to change in order to support changes to the protocol.
* Minimizes the volume of USBTMC interoperability specification material that has to be written and agreed to.
* Multiple protocols may be layered above a pass-through driver.
* Enables using a native pass-through driver if and when it exists.

The sections below describe specific behaviors for each system call. All USB Host USBTMC kernel drivers loaded for Class=0xFE, Subclass=0x03 devices must implement the system call behaviors defined below.

## CreateFile()

Parameters and behaviors are as specified in the Windows documentation.

In addition, for USBTMC, CreateFile() will open transfer pipes to the control endpoint and to each of the USBTMC interface endpoints.

The actual filename of the kernel driver is irrelevant. In other words, user-level client USBTMC code should not be searching for a specific filename. The correct way to find USBTMC resources is to use the class GUID reserved for USBTMC. Windows defines the routines necessary to query kernel filenames that can be passed to CreateFile().

The algorithm for finding all available USBTMC kernel filenames is to first call SetupDiGetClassDevs. This returns a handle to be used with the remaining calls. In a loop, you call SetupDiEnumDeviceInterfaces and SetupDiGetDeviceInterfaceDetail. The SP\_INTERFACE\_DEVICE\_DETAIL\_DATA structure gives you the kernel filename to pass to CreateFile(). Finally, release the class handle with the function SetupDiDestroyDeviceInfoList.

A VISA I/O library must always set FILE\_FLAG\_OVERLAPPED when calling CreateFile(). This is required for waiting on interrupt data while simultaneously performing normal I/O.

In reality, the kernel driver does not know and should not care whether the user calls CreateFile() with or without FILE\_FLAG\_OVERLAPPED. This text is here mainly for clarification.

The USBTMC kernel driver allows multiple handles to a device to be active at any time.

## WriteFile()

Parameters and behaviors are as specified in the Windows documentation.

In addition, for USBTMC, the data in the buffer passed in is sent unmodified to the bulk-OUT endpoint associated with the file handle.

The implementation of WriteFile() must support transferring data buffers that are larger than the internal maximum transfer size. For example, if the internal USB buffer is 8KB, and the user buffer is 30KB, then the implementation of WriteFile() must transfer the entire user buffer by looping over the buffer (in this case 4 times) and sending a portion from the user buffer each time. The implementation of WriteFile() may send less than the entire transfer count only if an error occurs.

Regardless of whether the user called CreateFile() with FILE\_FLAG\_OVERLAPPED, the USBTMC kernel implementation of WriteFile() must be able to implement requests asynchronously, in other words, it must be capable of returning STATUS\_PENDING. This is not a requirement for all transfer sizes, in other words, it is valid for a USBTMC kernel implementation to perform tiny transfers synchronously. Note that if the user did not call CreateFile() with FILE\_FLAG\_OVERLAPPED, the operating system will cause the call to WriteFile() to block until the USBTMC kernel driver marks the IRP as complete.

## ReadFile()

Parameters and behaviors are as specified in the Windows documentation.

In addition, for USBTMC, the data received is placed into the specified buffer and is returned unmodified.

ReadFile() must return if a non-maximum length packet is received or the amount of data requested has been received.

The implementation of ReadFile() must support transferring data buffers that are larger than the internal maximum transfer size. For example, if the internal USB buffer is 8KB, and the user buffer is 30KB, then the implementation of ReadFile() must transfer the entire user buffer by looping over the buffer (in this case 4 times) and reading a portion into the user buffer each time. The implementation of ReadFile() may read less than the entire transfer count only if an error occurs or it receives a short packet.

Regardless of whether the user called CreateFile() with FILE\_FLAG\_OVERLAPPED, the USBTMC kernel implementation of ReadFile() must be able to implement requests asynchronously, in other words, it must be capable of returning STATUS\_PENDING. This is not a requirement for all transfer sizes, in other words, it is valid for a USBTMC kernel implementation to perform tiny transfers synchronously. Note that if the user did not call CreateFile() with FILE\_FLAG\_OVERLAPPED, the operating system will cause the call to ReadFile() to block until the USBTMC kernel driver marks the IRP as complete.

## DeviceIoControl()

Parameters and behaviors are as specified in the Windows documentation.

In addition, for USBTMC, drivers must support the following IOCTL codes. See also section 3.

|  |  |  |
| --- | --- | --- |
|  | | |
| IOCTL macro | Value | Description |
| IOCTL\_USBTMC\_GETINFO | 0x8000\_2000 | Gets information about the Windows USB Host USBTMC driver. |
| IOCTL\_USBTMC\_CANCEL\_IO | 0x8000\_2004 | Cancels all IRPs on caller-designated pipe. |
| IOCTL\_USBTMC\_WAIT\_INTERRUPT | 0x8000\_2008 | Waits for data to arrive on interrupt-IN endpoint. If overlapped, the overlapped event is set when interrupt-IN DATA is received. |
| IOCTL\_USBTMC\_RESET\_PIPE | 0x8000\_201C | Clears a Halt condition on a pipe. |
| IOCTL\_USBTMC\_SEND\_REQUEST | 0x8000\_2080 | Sends an arbitrary request to the device control endpoint. |
| IOCTL\_USBTMC\_GET\_LAST\_ERROR | 0x8000\_2088 | Gets the most recent error returned from the lower-level USB driver. |

Table ‑ -- USBTMC IOCTL codes

All DeviceIoControl() requests have the following parameters.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | | | |
| Parameter Type | Parameter Name | Description |
| HANDLE | hDevice | Device handle, obtained by calling CreateFile. |
| DWORD | dwControlCode | Operation control code. One of the IOCTL’s in Table 1. |
| LPVOID | lpInBuffer | Input data buffer |
| DWORD | nInBufferSize | Size of input data buffer |
| DWORD | lpOutBuffer | Output data buffer |
| DWORD | nOutBufferSize | Size of output data buffer |
| LPDWORD | lpBytesReturned | Pointer to a location to receive the number of bytes returned. |
| LPOVERLAPPED | lpOverlapped | Optional pointer to an OVERLAPPED structure (described in the Windows Platform SDK documentation). |

Table ‑ -- DeviceIoControl parameters

### IOCTL\_USBTMC\_GETINFO

Returns information about the USBTMC driver.

|  |  |  |  |
| --- | --- | --- | --- |
|  | | | |
| Parameter Name | Description |
| hDevice | Device handle, obtained by calling CreateFile. |
| dwControlCode | IOCTL\_USBTMC\_GETINFO |
| lpInBuffer | NULL |
| nInBufferSize | 0 |
| lpOutBuffer | Output data buffer. Pointer to a USBTMC\_DRV\_INFO structure. |
| nOutBufferSize | Size of output data buffer. Must be sizeof(USBTMC\_DRV\_INFO). |
| lpBytesReturned | | Pointer to a location to receive the number of bytes returned. |
| lpOverlapped | | Optional pointer to an OVERLAPPED structure (described in the Windows Platform SDK documentation). |

When the DeviceloControl function is called with the IOCTL\_USBTMC\_GETINFO I/O control code, the caller must specify the address of a USBTMC\_DRV\_INFO structure as the function's lpOutBuffer parameter. The kernel-mode driver fills in the structure members.

**Code Example**

USBTMC\_DRV\_INFO drvrInfo;

DWORD cbRet;

**OVERLAPPED overlapped;**

BOOL bRet;

memset(&overlapped, 0, sizeof(OVERLAPPED));

overlapped.hEvent = CreateEvent(NULL, FALSE, FALSE, NULL);

bRet = DeviceIoControl( DeviceHandle,

(DWORD) IOCTL\_USBTMC\_GETINFO,

NULL,

0,

&drvInfo,

sizeof(USBTMC\_DRV\_INFO),

&cbRet,

&overlapped);

if( bRet == TRUE )

WaitForSingleObject(overlapped.hEvent, INFINITE);

CloseHandle(overlapped.hEvent);

#### Data structure – USBTMC\_DRV\_INFO

typedef struct {

DWORD major; // major revision of driver

DWORD minor; // minor revision of driver

DWORD build; // internal build number

WCHAR manufacturer[64]; // unicode manufacturer string

} USBTMC\_DRV\_INFO, \*PUSBTMC\_DRV\_INFO;

As with all Unicode strings, the manufacturer field must be NULL-terminated. This field can contain any valid Unicode character, and this specification does not impose any further restrictions.

Note that this entire data structure (USBTMC\_DRV\_INFO) and its IOCTL (IOCTL\_USBTMC\_GETINFO) are for diagnostic purposes. If a future Microsoft pass-through driver does not support this IOCTL or all of its fields, USBTMC client software should not be severely affected. USBTMC client software should not rely on any part of this IOCTL for normal and proper operation.

### IOCTL\_USBTMC\_CANCEL\_IO

This IOCTL cancels activity on the specified USB transfer pipe that is associated with the specified device handle.

|  |  |  |
| --- | --- | --- |
|  | | |
| Parameter Name | Description |
| hDevice | Device handle, obtained by calling CreateFile. |
| dwControlCode | IOCTL\_USBTMC\_CANCEL\_IO |
| lpInBuffer | Pointer to a location containing a USBTMC\_PIPE\_TYPE-typed value |
| nInBufferSize | Sizeof(USBTMC\_PIPE\_TYPE) |
| lpOutBuffer | NULL |
| nOutBufferSize | 0 |
| lpBytesReturned | 0 |
| lpOverlapped | Optional pointer to an OVERLAPPED structure (described in the Windows Platform SDK documentation). |

When the DeviceloControl function is called with the IOCTL\_USBTMC\_CANCEL\_IO I/O control code, the caller must specify one of the [USBTMC\_PIPE\_TYPE](#_Data_Structures_–)-typed values as the function's lpInBuffer parameter. This value indicates on which of the transfer pipes (interrupt, bulk IN, bulk OUT) the operation should be performed.

The driver creates an URB with function = URB\_FUNCTION\_ABORT\_PIPE to carry out the request.

**Code Example**

BOOL bState = FALSE;

DWORD cbRet = 0;

OVERLAPPED overlapped;

memset(&overlapped, 0, sizeof(OVERLAPPED));

overlapped.hEvent =

CreateEvent(NULL, // pointer to security attributes

FALSE, // automatic reset

FALSE, // initialize to nosignaled

NULL); // pointer to the event-object name

bState =

DeviceIoControl(hdlDevice,

(DWORD) IOCTL\_USBTMC\_CANCEL\_IO,

(LPVOID)&pipeType,

sizeof([USBTMC\_PIPE\_TYPE](#_Data_Structures_–)),

NULL,

0,

&cbRet,

&overlapped);

#### Data Structures – USBTMC\_PIPE\_TYPE

typedef enum {

USBTMC\_INTERRUPT\_IN\_PIPE = 1,

USBTMC\_READ\_DATA\_PIPE = 2,

USBTMC\_WRITE\_DATA\_PIPE = 3,

USBTMC\_ALL\_PIPES = 4

} USBTMC\_PIPE\_TYPE;

The USBTMC\_PIPE\_TYPE data type is used as input to the DeviceIoControl function, if the I/O control code is IOCTL\_USBTMC\_CANCEL\_IO or IOCTL\_USBTMC\_RESET\_PIPE. An interrupt pipe, a bulk IN pipe, and a bulk OUT pipe are associated with each device handle supplied to DeviceIoControl. The specified [USBTMC\_PIPE\_TYPE](#_Data_Structures_–) value indicates on which of these pipes the operation should be performed.

### IOCTL\_USBTMC\_WAIT\_INTERRUPT

Returns data arriving on a USB interrupt pipe.

|  |  |
| --- | --- |
|  | |
| Parameter Name | Description |
| hDevice | Device handle, obtained by calling CreateFile. |
| dwControlCode | IOCTL\_USBTMC\_WAIT\_INTERRUPT |
| lpInBuffer | NULL |
| nInBufferSize | 0 |
| lpOutBuffer | Pointer to a buffer that is large enough to receive the largest packet the device is capable of sending on the interrupt pipe. May be large enough to receive several packets. |
| nOutBufferSize | Size of the output buffer. |
| lpBytesReturned | Pointer to a location to receive the number of bytes returned. |
| lpOverlapped | Optional pointer to an OVERLAPPED structure (described in the Windows Platform SDK documentation). |

Any application process or thread can issue a DeviceIoControl() with IOCTL\_USBTMC\_  
WAIT\_INTERRUPT. The USBTMC kernel driver distributes interrupt-IN DATA to multiple processes. A VISA I/O library may issue a new IOCTL\_USBTMC\_WAIT\_INTERRUPT if one is already outstanding for a given USBTMC interface.

**Code Example**

DWORD dwError;

BOOL bRet;

BYTE InterruptData[64];

OVERLAPPED overlappedIntIn;

memset(&overlappedIntIn, 0, sizeof(overlappedIntIn));

overlappedIntIn.hEvent = CreateEvent( NULL, TRUE, FALSE, NULL );

bRet = DeviceIoControl( hHandle,

IOCTL\_USBTMC\_WAIT\_INTERRUPT,

NULL,

0,

&InterruptData,

sizeof(InterruptData),

&dwError,

&overlappedIntIn );

if ( bRet != 0 ) {

printf("DeviceIoControl err\n");

}

WaitForSingleObject(overlappedIn.hEvent,INFINITE);

### IOCTL\_USBTMC\_RESET\_PIPE

Resets the specified USB transfer pipe that is associated with the specified device handle. This clears a Halt condition on the pipe.

|  |  |  |
| --- | --- | --- |
|  | | |
| Parameter Name | Description | |
| hDevice | Device handle, obtained by calling CreateFile. | |
| dwControlCode | IOCTL\_USBTMC\_RESET\_PIPE | |
| lpInBuffer | NULL | |
| nInBufferSize | 0 | |
| lpOutBuffer | Pointer to a location containing a [USBTMC\_PIPE\_TYPE](#_Data_Structures_–)-typed value. | |
| nOutBufferSize | Size of the output buffer. | |
| lpBytesReturned | Pointer to a location to receive the number of bytes returned. | |
| lpOverlapped | Optional pointer to an OVERLAPPED structure (described in the Windows Platform SDK documentation). | |

When the DeviceloControl function is called with the IOCTL\_USBTMC\_RESET\_PIPE I/O control code, the caller must specify one of the [USBTMC\_PIPE\_TYPE](../../../../AppData/USBTMC/stifnc_1wo9.htm)-typed values as the function's lpInBuffer parameter. This value indicates on which of the transfer pipes (interrupt, bulk IN, bulk OUT) the operation should be performed.

The driver creates an URB with function = URB\_FUNCTION\_RESET\_PIPE to carry out the request.

### IOCTL\_USBTMC\_SEND\_REQUEST

Sends a vendor-defined or class-specific request to a USB device, using the control pipe, and optionally sends or receives additional data.

|  |  |  |
| --- | --- | --- |
|  | | |
| Parameter Name | Description | |
| hDevice | Device handle, obtained by calling CreateFile. | |
| dwControlCode | IOCTL\_USBTMC\_SEND\_REQUEST | |
| lpInBuffer | Pointer to an [USBTMC\_IO\_BLOCK](../../../../AppData/USBTMC/stifnc_0pbd.htm) structure. | |
| nInBufferSize | Sizeof(USBTMC\_IO\_BLOCK) | |
| lpOutBuffer | Pointer to the same buffer identified by the PbyData member of the USBTMC\_IO\_BLOCK structure, or NULL if a data transfer is not being requested. | |
| nOutBufferSize | Size of the output buffer, or zero if a data transfer is not being requested. | |
| lpBytesReturned | Pointer to a location to receive the number of bytes returned. | |
| lpOverlapped | Optional pointer to an OVERLAPPED structure (described in the Windows Platform SDK documentation). | |

When the DeviceloControl function is called with the IOCTL\_USBTMC\_SEND\_REQUEST control code, the caller must specify the address of an [USBTMC\_IO\_BLOCK](#_Data_Structure_–_2) structure as the function's lpInBuffer parameter. The type of request specified with this I/O control code is device-specific and vendor-defined, as are the type and size of any information that might be sent or received.

The USBTMC kernel implementation must support all vendor-specific requests. For class-specific requests, if the Windows operating system implements a given request, then the USBTMC kernel implementation must support that request. If the Windows operating system does not define an implementation for a given request, such as if the bmRequestType or bRequest parameter is an undefined class request, then the USBTMC kernel implementation must return the error STATUS\_INVALID\_PARAMETER.

The following table shows how input arguments should be specified.

|  |  |  |  |
| --- | --- | --- | --- |
|  | | | |
|  | Read Operation | Write Operation | No data transfer |
| lpInBuffer | USBTMC\_IO\_BLOCK pointer. | USBTMC\_IO\_BLOCK pointer. | USBTMC\_IO\_BLOCK pointer. |
| lpOutBuffer | Pointer to buffer that will receive data to be read. | Pointer to buffer containing data to be written. | NULL |
| lpOutBufferSize | Size of buffer. | Size of buffer. | Zero |
| pbyData member of USBTMC\_IO\_BLOCK | Same pointer as lpOutBuffer. | Same pointer as lpOutBuffer. | NULL |
| wLength member of USBTMC\_IO\_BLOCK | Same value as lpOutBufferSize. | Same value as lpOutBufferSize. | Zero |
| fTransferDirectionIn member of USBTMC\_IO\_BLOCK | TRUE | FALSE | FALSE |

#### Data Structure – USBTMC\_IO\_BLOCK

The USBTMC\_IO\_BLOCK structure is used as a parameter to DeviceIoControl, when the specified I/O control code is IOCTL\_USBTMC\_SEND\_REQUEST. Values contained in structure members are used to create a USB Device Request (described in the Universal Serial Bus Specification).

typedef struct {

IN unsigned char bmRequestType;

IN unsigned char bRequest;

IN unsigned short wValue;

IN unsigned short wIndex;

IN unsigned short wLength;

IN OUT PUCHAR pbyData;

IN UCHAR fTransferDirectionIn;

} USBTMC\_IO\_BLOCK, \*PUSBTMC\_IO\_BLOCK;

|  |  |
| --- | --- |
| USBTMC\_IO\_BLOCK field | Usage |
| bmRequestType | Used as the Setup DATA bmRequestType |
| bRequest | Used as the Setup DATA bRequest |
| wValue | Used as the Setup DATA wValue |
| wIndex | Used as the Setup DATA wIndex |
| wLength | Used as the Setup DATA wLength |
| pbyData | Pointer to a data buffer with a length of wLength. |
| fTransferDirectionIn | TRUE for transfers from device to host; FALSE for transfers from host to device. |

The following rules apply when using this data structure:

* pbyData must match lpOutBuffer. If it does not match, ensuing behavior is not guaranteed.
* fTransferDirectionIn must be 0 for a write (data transfer direction = OUT) operation and must be 1 for a read (data transfer direction = IN) operation. Must match direction in bmRequestType. If it does not match, ensuing behavior is not guaranteed.

### IOCTL\_USBTMC\_GET\_LAST\_ERROR

Gets the last error code returned from the lower-level USB driver.

|  |  |
| --- | --- |
| Parameter Name | Description |
| hDevice | Device handle, obtained by calling CreateFile. |
| dwControlCode | IOCTL\_USBTMC\_GET\_LAST\_ERROR |
| lpInBuffer | NULL |
| nInBufferSize | 0 |
| lpOutBuffer | Output data buffer. Pointer to a USBD\_STATUS. |
| nOutBufferSize | Size of output data buffer. Must be **sizeof(USBD\_STATUS)**. |
| lpBytesReturned | Pointer to a location to receive the number of bytes returned. |
| lpOverlapped | Optional pointer to an OVERLAPPED structure (described in the Windows Platform SDK documentation). |

When the DeviceloControl function is called with the IOCTL\_USBTMC\_GET\_LAST\_ERROR I/O control code, the caller must specify the address of a USBD\_STATUS value as the function's lpOutBuffer parameter. The kernel-mode driver fills in the value with the last error code that it received from USBD.

If the USBTMC kernel driver has never encountered a USBD error, this output value must be 0. The USBTMC kernel driver must not change this value when it returns an error code other than a USBD error. Querying the last error does not cause the USBTMC kernel to reset the cached error code value.

## CloseHandle()

Parameters and behaviors are as specified in the Windows documentation.

## INF files for USBTMC devices

INF files determine the kernel driver associated with a USBTMC device. INF files also determine where USBTMC devices show up in the Windows “Device Manager”.

### Class and ClassGUID for USBTMC devices

None of the existing Windows device setup classes apply to USBTMC devices. A USBTMC INF file may define a new device setup class for USBTMC devices. The Class and ClassGUID fields appropriate for USBTMC devices are shown below.

[Version]

...

Class=%USBTMC\_CLASS%

ClassGUID=%USBTMC\_GUID%

...

[Strings]  
USBTMC\_CLASS="USBTestAndMeasurementDevice"  
USBTMC\_GUID="{A9FDBB24-128A-11d5-9961-00108335E361}"

### INF ClassInstall32 section

An INF file for USBTMC devices may have a [ClassInstall] section to add a class description and a class icon to the registry. An example of INF file content to accomplish this is shown below.

…

[ClassInstall32]

AddReg=UsbTmcAddReg

…

[UsbTmcAddReg]

HKR,,,%UsbTmcDevClassName%

HKR,,Icon,,-20

…

[Strings]

UsbTmcDevClassName=”USB Test and Measurement Devices”

…

The example above uses icon number -20. This is a standard icon for the Windows device manager for USB devices. It has existed since Windows 98 and works on all current Windows WDM operating systems. A vendor is allowed to use a different icon as long as they provide the Windows resource for it.

### INF DDInstall.Interfaces section

An INF file for USBTMC devices may have a [DDInstall.Interfaces] section to add the DeviceClasses\{InterfaceClassGUID} to the registry. {InterfaceClassGUID} is the same as the ClassGUID above. Note that the use of the term DDInstall here is a placeholder for an install section name in the vendor’s INF file.

[install-section-name.Interfaces]

AddInterface=%USBTMC\_GUID%

### Product specific INF files

Any vendor may supply product specific INF files for USBTMC device(s). An example of part of such an INF file is shown below.

…

[Models]

device-description = install-section-name, USB\Vid\_XX&Pid\_YY

device-description = install-section-name, USB\Vid\_XX&Pid\_ZZ

…

where

* XX is the idVendor in the device descriptor
* YY is the idProduct in the device descriptor for product #1
* ZZ is the idProduct in the device descriptor for product #2

Any software that installs a product specific INF file must also install all of the necessary files required by the INF file.

### Class, SubClass, Protocol specific INF files

Any vendor may supply an INF file generic to a set of USBTMC devices with the same bInterfaceClass, bInterfaceSubClass, and bInterfaceProtocol. This mechanism provides a way for a vendor to override operating system vendor supplied INF files for USBTMC devices. An example of part of such an INF file is shown below.

…

[Models]

device-description = install-section-name, USB\Class\_XX&SubClass\_YY&Prot\_ZZ

…

where

* XX is the bInterfaceClass in the interface descriptor
* YY is the bInterfaceSubClass in the interface descriptor
* ZZ is the bInterfaceProtocol in the interface descriptor

Any software that installs a class, subclass, and protocol specific INF file must also install all of the necessary files required by the INF file.

### Class, SubClass specific INF files and Class specific INF files

Only the operating system vendor is allowed to supply an INF file generic to a set of USBTMC devices with the same bInterfaceClass and bInterfaceSubClass. An example of part of such an INF file is shown below.

…

[Models]

device-description = install-section-name, USB\Class\_XX&SubClass\_YY

…

where

* XX is the bInterfaceClass in the interface descriptor
* YY is the bInterfaceSubClass in the interface descriptor

Table ‑ -- INF file syntax permissions

|  |  |  |  |
| --- | --- | --- | --- |
| INF file syntax: | Operating System Vendor  (eg. Microsoft) | VISA I/O Library Vendor | Instrument Vendor |
| Class\_##&Subclass\_## | Yes | No | No |
| Class\_##&Subclass\_##&Prot\_## | No | Yes | No |
| Vid\_## | No | No | Yes |
| Vid\_##&Pid\_## | No | No | Yes |

# USBTMC include file

The following content summarizes the content that must be placed in a header file associated with the USBTMC kernel driver.

#ifndef USBTMC\_IOCTL\_H

#define USBTMC\_IOCTL\_H

#include <windows.h>

#include <devioctl.h>

//===================================================================

// The following are the I/O control codes that this driver supports.

#define FILE\_DEVICE\_USBTMC 0x8000

#define IOCTL\_INDEX 0x0800

#define IOCTL\_USBTMC(idx,meth) CTL\_CODE(FILE\_DEVICE\_USBTMC,(idx),(meth),FILE\_ANY\_ACCESS)

#define IOCTL\_USBTMC\_GETINFO IOCTL\_USBTMC(IOCTL\_INDEX, METHOD\_BUFFERED) // 0x80002000

#define IOCTL\_USBTMC\_CANCEL\_IO IOCTL\_USBTMC(IOCTL\_INDEX+1, METHOD\_BUFFERED) // 0x80002004

#define IOCTL\_USBTMC\_WAIT\_INTERRUPT IOCTL\_USBTMC(IOCTL\_INDEX+2, METHOD\_BUFFERED) // 0x80002008

#define IOCTL\_USBTMC\_RESET\_PIPE IOCTL\_USBTMC(IOCTL\_INDEX+7, METHOD\_BUFFERED) // 0x8000201C

#define IOCTL\_USBTMC\_SEND\_REQUEST IOCTL\_USBTMC(IOCTL\_INDEX+32,METHOD\_BUFFERED) // 0x80002080

#define IOCTL\_USBTMC\_GET\_LAST\_ERROR IOCTL\_USBTMC(IOCTL\_INDEX+34,METHOD\_BUFFERED) // 0x80002088

//=======================================================================

// The following are required data structures used for DeviceIoControl.

// Applications will pass data to the driver using these data structures.

// This data structure is used for:

// IOCTL\_USBTMC\_SEND\_REQUEST

typedef struct USBTMC\_IO\_BLOCK

{

UCHAR bmRequestType;

UCHAR bRequest;

USHORT wValue;

USHORT wIndex;

USHORT wLength;

PUCHAR pbyData; // ignore – use lpOutBuffer instead – usbscan compatible

UCHAR fTransferDirectionIn; // ignore – use bmRequestType instead – usbscan compatible

} USBTMC\_IO\_BLOCK, \*PUSBTMC\_IO\_BLOCK;

// This data structure is used for:

// IOCTL\_USBTMC\_CANCEL\_IO

// IOCTL\_USBTMC\_RESET\_PIPE

typedef enum USBTMC\_PIPE\_TYPE

{

USBTMC\_INTERRUPT\_IN\_PIPE = 1,

USBTMC\_READ\_DATA\_PIPE = 2,

USBTMC\_WRITE\_DATA\_PIPE = 3,

USBTMC\_ALL\_PIPES = 4

} USBTMC\_PIPE\_TYPE, \*PUSBTMC\_PIPE\_TYPE;

// This data structure is used for:

// IOCTL\_USB\_GETINFO

typedef struct USBTMC\_DRV\_INFO

{

USHORT major;

USHORT minor;

USHORT build;

WCHAR manufacturer[64];

} USBTMC\_DRV\_INFO, \*PUSBTMC\_DRV\_INFO;

//============================================================================

// Class GUID for all USBTMC devices is {A9FDBB24-128A-11D5-9961-00108335E361}

#define USBTMC\_CLASS\_GUID (GUID)\

{ 0xa9fdbb24, 0x128a, 0x11d5, { 0x99, 0x61, 0x00, 0x10, 0x83, 0x35, 0xe3, 0x61 } }

#endif

# Available USBD Functions

Not all “Standard Request Codes” listed in Table 9.4 of the Universal Serial Bus Specification are supported by USBD. Following is an excerpt from usbdi.h, the header file that defines function codes and error codes for USBD:

#define URB\_FUNCTION\_SELECT\_CONFIGURATION 0x0000

#define URB\_FUNCTION\_SELECT\_INTERFACE 0x0001

#define URB\_FUNCTION\_ABORT\_PIPE 0x0002

#define URB\_FUNCTION\_TAKE\_FRAME\_LENGTH\_CONTROL 0x0003

#define URB\_FUNCTION\_RELEASE\_FRAME\_LENGTH\_CONTROL 0x0004

#define URB\_FUNCTION\_GET\_FRAME\_LENGTH 0x0005

#define URB\_FUNCTION\_SET\_FRAME\_LENGTH 0x0006

#define URB\_FUNCTION\_GET\_CURRENT\_FRAME\_NUMBER 0x0007

#define URB\_FUNCTION\_CONTROL\_TRANSFER 0x0008

#define URB\_FUNCTION\_BULK\_OR\_INTERRUPT\_TRANSFER 0x0009

#define URB\_FUNCTION\_ISOCH\_TRANSFER 0x000A

#define URB\_FUNCTION\_RESET\_PIPE 0x001E

// These functions correspond to the standard commands on

// the default pipe. The direction is implied.

#define URB\_FUNCTION\_GET\_DESCRIPTOR\_FROM\_DEVICE 0x000B

#define URB\_FUNCTION\_GET\_DESCRIPTOR\_FROM\_ENDPOINT 0x0024

#define URB\_FUNCTION\_GET\_DESCRIPTOR\_FROM\_INTERFACE 0x0028

#define URB\_FUNCTION\_SET\_DESCRIPTOR\_TO\_DEVICE 0x000C

#define URB\_FUNCTION\_SET\_DESCRIPTOR\_TO\_ENDPOINT 0x0025

#define URB\_FUNCTION\_SET\_DESCRIPTOR\_TO\_INTERFACE 0x0029

#define URB\_FUNCTION\_SET\_FEATURE\_TO\_DEVICE 0x000D

#define URB\_FUNCTION\_SET\_FEATURE\_TO\_INTERFACE 0x000E

#define URB\_FUNCTION\_SET\_FEATURE\_TO\_ENDPOINT 0x000F

#define URB\_FUNCTION\_SET\_FEATURE\_TO\_OTHER 0x0023

#define URB\_FUNCTION\_CLEAR\_FEATURE\_TO\_DEVICE 0x0010

#define URB\_FUNCTION\_CLEAR\_FEATURE\_TO\_INTERFACE 0x0011

#define URB\_FUNCTION\_CLEAR\_FEATURE\_TO\_ENDPOINT 0x0012

#define URB\_FUNCTION\_CLEAR\_FEATURE\_TO\_OTHER 0x0022

#define URB\_FUNCTION\_GET\_STATUS\_FROM\_DEVICE 0x0013

#define URB\_FUNCTION\_GET\_STATUS\_FROM\_INTERFACE 0x0014

#define URB\_FUNCTION\_GET\_STATUS\_FROM\_ENDPOINT 0x0015

#define URB\_FUNCTION\_GET\_STATUS\_FROM\_OTHER 0x0021

// Direction is specified in TransferFlags.

#define URB\_FUNCTION\_RESERVED0 0x0016

// These are for sending vendor and class commands on the

// default pipe. The direction is specified in TransferFlags.

#define URB\_FUNCTION\_VENDOR\_DEVICE 0x0017

#define URB\_FUNCTION\_VENDOR\_INTERFACE 0x0018

#define URB\_FUNCTION\_VENDOR\_ENDPOINT 0x0019

#define URB\_FUNCTION\_VENDOR\_OTHER 0x0020

#define URB\_FUNCTION\_CLASS\_DEVICE 0x001A

#define URB\_FUNCTION\_CLASS\_INTERFACE 0x001B

#define URB\_FUNCTION\_CLASS\_ENDPOINT 0x001C

#define URB\_FUNCTION\_CLASS\_OTHER 0x001F

// Reserved function codes.

#define URB\_FUNCTION\_RESERVED 0x001D

#define URB\_FUNCTION\_GET\_CONFIGURATION 0x0026

#define URB\_FUNCTION\_GET\_INTERFACE 0x0027

#define URB\_FUNCTION\_LAST 0x0029

Upon mapping Table 9-4 onto the above function codes defined for USBD, the following “Required USBD Function Code Support” table becomes apparent. These mappings of bmRequestType and bmRequest to USB’s are required:

|  |  |  |  |
| --- | --- | --- | --- |
|  | | | |
| **Table 4‑1: Required USBD Function Code Support** | | | |
| **Required USBD Function Code Support** | | | |
| **bmRequestType (with value)** | **bRequest**  **(with value)** | **Recipient (with value)** | |
| Class (0x20) | NA | DEVICE (0) | URB\_FUNCTION\_CLASS\_DEVICE (0x001A) |
| INTERFACE (1) | URB\_FUNCTION\_CLASS\_INTERFACE (0x001B) |
| ENDPOINT (2) | URB\_FUNCTION\_CLASS\_ENDPOINT (0x001C) |
| OTHER (3) | URB\_FUNCTION\_CLASS\_OTHER (0x001F) |
| Vendor (0x40) | NA | DEVICE (0) | URB\_FUNCTION\_VENDOR\_DEVICE (0x0017) |
| INTERFACE (1) | URB\_FUNCTION\_VENDOR\_INTERFACE (0x0018) |
| ENDPOINT (2) | URB\_FUNCTION\_VENDOR\_ENDPOINT (0x0019) |
| OTHER (3) | URB\_FUNCTION\_VENDOR\_OTHER (0x0020) |
| Reserved (0x60) | NA | URB\_FUNCTION\_RESERVED (0x001D) | |
| Standard (0x00) | GET\_STATUS (0) | DEVICE (0) | URB\_FUNCTION\_GET\_STATUS\_FROM\_DEVICE (0x0013) |
| INTERFACE (1) | URB\_FUNCTION\_GET\_STATUS\_FROM\_INTERFACE (0x0014) |
| ENDPOINT (2) | URB\_FUNCTION\_GET\_STATUS\_FROM\_ENDPOINT (0x0015) |
| OTHER (3) | URB\_FUNCTION\_GET\_STATUS\_FROM\_OTHER (0x0021) |
| CLEAR\_FEATURE (1) | DEVICE (0) | URB\_FUNCTION\_CLEAR\_FEATURE\_TO\_DEVICE (0x0010) |
| INTERFACE (1) | URB\_FUNCTION\_CLEAR\_FEATURE\_TO\_INTERFACE (0x0011) |
| ENDPOINT (2) | URB\_FUNCTION\_CLEAR\_FEATURE\_TO\_ENDPOINT (0x0012) |
| OTHER (3) | URB\_FUNCTION\_CLEAR\_FEATURE\_TO\_OTHER (0x0022) |
| SET\_FEATURE  (3) | DEVICE (0) | URB\_FUNCTION\_SET\_FEATURE\_TO\_DEVICE (0x000D) |
| INTERFACE (1) | URB\_FUNCTION\_SET\_FEATURE\_TO\_INTERFACE (0x000E) |
| ENDPOINT (2) | URB\_FUNCTION\_SET\_FEATURE\_TO\_ENDPOINT (0x000F) |
| OTHER (3) | URB\_FUNCTION\_SET\_FEATURE\_TO\_OTHER (0x0023) |
| GET\_DESCRIPTOR (6) | DEVICE (0) | URB\_FUNCTION\_GET\_DESCRIPTOR\_FROM\_DEVICE (0x000B) |
| INTERFACE (1) | URB\_FUNCTION\_GET\_DESCRIPTOR\_FROM\_INTERFACE (0x0028) |
| ENDPOINT (2) | URB\_FUNCTION\_GET\_DESCRIPTOR\_FROM\_ENDPOINT (0x0024) |
| OTHER (3) | None |
| SET\_DESCRIPTOR (0x07) | DEVICE (0) | URB\_FUNCTION\_SET\_DESCRIPTOR\_TO\_DEVICE (0x000C) |
| INTERFACE (1) | URB\_FUNCTION\_SET\_DESCRIPTOR\_TO\_INTERFACE (0x0029) |
| ENDPOINT (2) | URB\_FUNCTION\_SET\_DESCRIPTOR\_TO\_ENDPOINT (0x0025) |
| OTHER (3) | None |
| GET\_CONFIGURATION (0x08) | DEVICE (0) | URB\_FUNCTION\_GET\_CONFIGURATION (0x0026) |
| INTERFACE (1) | None |
| ENDPOINT (2) | None |
| OTHER (3) | None |
| GET\_INTERFACE (0x0A) | DEVICE (0) | URB\_FUNCTION\_GET\_INTERFACE (0x0027) |
| INTERFACE (1) | None |
| ENDPOINT (2) | None |
| OTHER (3) | None |

Appendix A: Linux Specific Information

The IVI Foundation is both contributing to and using the USBTMC kernel driver that is part of the Linux kernel open source project.

This appendix is informational only. Because the Linux open source USBTMC kernel driver is not owned by the IVI Foundation, this specification does not specify the driver. However, this section documents changes contributed by the IVI Foundation to the Linux open source USBTMC kernel driver to make sure that IVI members can properly evaluate future proposed changes to the driver.

A.1 History

As part of the initial effort to migrate VISA standards to Linux in 2018, the IVI Foundation agreed that the best USBTMC solution on Linux was to use the existing Linux open source USBTMC kernel driver, if it could be modified to provide essential functionality from the Windows version of the driver. As a result, member companies contributed engineering time to modify and test the driver, and submitted their changes to the Linux kernel open source.

A.2 Added Features

In contrast to the Windows driver, the I/O operations of the initial Linux USBTMC kernel driver already include the USBTMC protocol header. Thus all contributed Linux kernel patches should still support current Linux applications and shall meet the following requirements needed for a VISA Library:

* Synchronous and asynchronous I/O operations
* Vendor specific and generic USB request operations
* Multiple applications can share access to the same instruments
* The driver handles SRQ conflicts
* Simplify definition of device access rules (udev) for USBTMC devices

A.2.1 Changes to ioctl USBTMC488\_IOCTL\_READ\_STB

The ioctl function USBTMC488\_IOCTL\_READ\_STB reads the Status Byte of the connected instrument. The Linux kernel driver supports USB488 interfaces with or without an Interrupt IN endpoint.

This function was modified to return the correct Status Byte with RQS bit set (Bit 6) when the instrument has issued a service request via Interrupt IN endpoint. If more file handles are opened to the same instrument, all file handles will receive the same status byte with RQS bit set. Note that instruments without Interrupt IN endpoint do not support SR1 device capabilities and will just return a Status Byte without RQS bit set.

A.2.2 Support for receiving SRQ notifications via poll/select

In many situations operations on multiple instruments need to be synchronized. The poll() and select() functions provide a convenient way of waiting on a number of different instruments and other peripherals simultaneously. When the instrument sends an SRQ notification the file descriptors (fd) watching for exceptional conditions become readable. To reset the exceptional condition a USBTMC488\_IOCTL\_READ\_STB ioctl must be performed.

With the new asynchronous functions the behavior of the poll function was extended.

* POLLPRI is set when the interrupt pipe receives a status byte with SRQ.
* POLLIN | POLLRDNORM signals that asynchronous URBs are available on IN pipe.
* POLLOUT | POLLWRNORM signals that no URBS are submitted to IN or OUT pipe. It is safe to write.
* POLLERR is set when any submitted URB fails.

Note that POLLERR cannot be masked out. That means waiting only for POLLPRI does not work when asynchronous operations are used. In this case using the next ioctl USBTMC488\_IOCTL\_WAIT\_SRQ is recommended.

A.2.3 New ioctl USBTMC488\_IOCTL\_WAIT\_SRQ

The new ioctl offers an alternative way to wait for a Service Request. In contrast to the poll() function (see above) the ioctl does not return when asynchronous operations fail.

The given parameter of type \_\_u32 specifies the maximum timeout in milliseconds to wait for the next Service Request.

The ioctl returns 0 or -1 with errno set:

* 0 when an SRQ is received
* errno = ETIMEDOUT when timeout (in ms) is elapsed.
* errno = ENODEV when file handle is closed or device disconnected
* errno = EFAULT when device does not have an interrupt pipe.

A.2.4 New ioctl USBTMC488\_IOCTL\_TRIGGER

This ioctl was added to send a TRIGGER Bulk-OUT header according to the Subclass USB488 Specification.

A.2.5 New ioctls USBTMC\_IOCTL\_GET/SET\_TIMEOUT

These ioctls were added to set/get the I/O timeout in milliseconds for a specific file handle. The I/O timeout is used for write(), read(), and USBTMC488\_IOCTL\_READ\_STB operations.

By default the timeout is set to 5000 milliseconds for compatibility with current Linux applications. VISA implementations should change this timeout to the VISA default of 2000 milliseconds.

USBTMC\_IOCTL\_SET\_TIMEOUT will return with an error EINVAL if timeout is set to less than 100 milliseconds.

A.2.6 New ioctl USBTMC\_IOCTL\_CTRL\_REQUEST

This new ioctl USBTMC\_IOCTL\_CTRL\_REQUEST allows sending arbitrary requests on the control pipe. VISA implementations will use it to implement the VISA API functions: viUsbControlIn/Out.

The given parameter is of type:

struct usbtmc\_ctrlrequest {

struct usbtmc\_request req;

void \_\_user \*data; /\* pointer to data \*/

} \_\_attribute\_\_ ((packed));

where struct usbtmc\_request defines the standard setup control request:

struct usbtmc\_request {

\_\_u8 bRequestType;

\_\_u8 bRequest;

\_\_u16 wValue;

\_\_u16 wIndex;

\_\_u16 wLength;

} \_\_attribute\_\_ ((packed));

A.2.7 New ioctl USBTMC\_IOCTL\_EOM\_ENABLE

By default the EOM bit is set on the last transfer of a write() operation. This ioctl enables or disables setting the EOM bit for the next write() operation.

Will return with error EINVAL if given parameter eom is not 0 or 1.

A.2.8 New ioctl USBTMC\_IOCTL\_CONFIG\_TERMCHAR

Allows enabling/disabling terminating a read on reception of a termination character. The parameters are passed with the struct:

struct usbtmc\_termchar {

\_\_u8 term\_char;

\_\_u8 term\_char\_enabled;

} \_\_attribute\_\_ ((packed));

This ioctl controls the field *TermChar* and Bit 1 of field *bmTransferAttributes* of the REQUEST\_DEV\_DEP\_MSG\_IN BULK-OUT header. By default *TermCharEnabled* is false and *TermChar* is '\n' (0x0a).

Will return with error EINVAL if *TermCharEnabled* is not 0 or 1 or if attempting to enable *TermCharEnabled* when the device does not support terminating a read when a byte matches the specified *TermChar*.

A.2.9 New ioctl USBTMC\_IOCTL\_MSG\_IN\_ATTR

The ioctl function returns the specific field bmTransferAttributes of the last DEV\_DEP\_MSG\_IN Bulk-IN header. This header is received by the read() function. The meaning of the (u8) bitmap bmTransferAttributes is:

* Bit 0 = EOM flag is set when the last of a USBTMC message is received.
* Bit 1 = Is set when the last byte is a termchar (e.g. '\n').   
  Note that this bit is always zero when the device does not support termchar feature or when termchar detection is not enabled (see ioctl USBTMC\_IOCTL\_CONFIG\_TERMCHAR).

A.2.10 New ioctl USBTMC\_IOCTL\_WRITE

The ioctl function uses the following struct to send generic OUT bulk messages for synchronous and asynchronous write operation:

#define USBTMC\_FLAG\_ASYNC 0x0001

#define USBTMC\_FLAG\_APPEND 0x0002

struct usbtmc\_message {

\_\_u32 transfer\_size; /\* size of bytes to transfer \*/

\_\_u32 transferred; /\* size of received/written bytes \*/

\_\_u32 flags; /\* bit 0: 0 = synchronous; 1 = asynchronous \*/

void \_\_user \*message; /\* pointer to header and data in user space \*/

} \_\_attribute\_\_ ((packed));

In synchronous mode (flags=0) the generic write function sends the message with a size of transfer\_size. The message is split into chunks of 4k (=page size) and submitted (by usb\_submit\_urb) to the Bulk Out. A semaphore limits the number of flying urbs. The function waits for the end of transmission or returns on error, for example when a single chunk exceeds the timeout. The member usbtmc\_message.transferred returns the number of transferred bytes.

In asynchronous mode (flags=USBTMC\_FLAG\_ASYNC) the generic write function is non-blocking. The ioctl clears the current error state and the internal transfer counter. The member usbtmc\_message.transferred returns the number of submitted bytes, however less data can be sent to the device in case of error. The internal transfer counter holds the number of total transferred bytes.

With flag USBTMC\_FLAG\_APPEND additional urbs are submitted without clearing the current error state or internal transfer counter.

The function returns -1 and sets errno = EAGAIN when the semaphore does not allow submitting any urb.

POLLOUT | POLLWRNORM are signaled when all submitted urbs are completed. POLLERR is set when any urb fails. See poll() function above.

A.2.11 New ioctl USBTMC\_IOCTL\_WRITE\_RESULT

The ioctl function copies the current internal transfer counter to the given \_\_u32 pointer and returns the current error state of the last (asynchronous) USBTMC\_IOCTL\_WRITE call. The error state and internal transfer counter is not cleared by this ioctl.

A.2.12 New ioctl USBTMC\_IOCTL\_READ

The ioctl function uses the following struct to get generic IN bulk messages:

#define USBTMC\_FLAG\_ASYNC 0x0001

#define USBTMC\_FLAG\_IGNORE\_TRAILER 0x0004

struct usbtmc\_message {

\_\_u32 transfer\_size; /\* size of bytes to transfer \*/

\_\_u32 transferred; /\* size of received/written bytes \*/

\_\_u32 flags; /\* bit 0: 0 = synchronous; 1 = asynchronous \*/

void \_\_user \*message; /\* pointer to header and data in user space \*/

} \_\_attribute\_\_ ((packed));

In synchronous mode (flags=0) the generic read function copies maximum transfer\_size bytes of received data from Bulk IN to the usbtmc\_message.message pointer. Depending on transfer\_size the read function submits one (<=4kB) or more urbs (up to 16) to Bulk IN. For best performance, the read function copies bytes from one urb to the message buffer while other urbs still can receive data from the T&M device concurrently. The function waits for the end of transmission or returns on error or timeout. The member usbtmc\_message.transferred returns the number of received bytes.

For best performance, the requested transfer size should be a multiple of 4 kB. Please note that the driver has to round down the transfer\_size to a multiple of 4 kB when you use more than 4kB, since the driver does not cache or save unread data. The flag USBTMC\_FLAG\_IGNORE\_TRAILER can be used when the transmission size is already known. Then the driver does not round down the transfer\_size to a multiple of 4 kB, but does reserve extra space to receive the final short or zero length packet. Note that the instrument may send up to wMaxPacketSize - 1 bytes at the end of a message to avoid sending a zero-length packet.

In asynchronous mode (flags=USBTMC\_FLAG\_ASYNC) the generic read function is non-blocking. When no received data is available, the read function submits urbs as many as needed to receive transfer\_size bytes. However, the number of flying urbs (=4kB) is limited to 16 even with subsequent calls of this ioctl.

The message pointer can be NULL when no receiving data shall be returned. The function returns -EAGAIN when no data is available. -EINVAL is returned when data is available but the message pointer is NULL.

When available data is copied to a valid usbtmc\_message.message pointer the member usbtmc\_message.transferred returns the number of received bytes.

POLLIN | POLLRDNORM are signaled when at least one urb has completed with received data. POLLOUT | POLLWRNORM are signaled when all submitted urbs IN/OUT are completed. POLLERR is set when any urb fails. See poll() function above.

The function returns:

* 1 when a short or zero length packet is detected.
* 0 is returned when the transferred size is a multiple of wMaxPacketSize
* -1 and errno = EAGAIN: when no data can be read asynchronous.
* -1 and errno = EINVAL: when message pointer is invalid and data could be read.
* -1 and errno = ETIMEDOUT: when no data can be read synchronous (see USBTMC\_IOCTL\_SET\_TIMEOUT) Otherwise the ioctl always returns the very first error of submitted urbs.

A.2.13 New ioctl USBTMC\_IOCTL\_CANCEL\_IO

This ioctl function cancels USBTMC\_IOCTL\_READ/USBTMC\_IOCTL\_WRITE functions. Internal error states are set to -ECANCELED. A subsequent call to USBTMC\_IOCTL\_READ or USBTMC\_IOCTL\_WRITE\_RESULT will return -ECANCELED with information about current transferred data.[[1]](#footnote-2)

A.2.14 New ioctl USBTMC\_IOCTL\_CLEANUP\_IO

This ioctl function kills all submitted urbs to OUT and IN pipe, and clears all received data from IN pipe. The Internal transfer counters and error states are reset. An application should use this ioctl after an asynchronous transfer was canceled and/or error handling has finished.

A.2.15 New ioctl USBTMC\_IOCTL\_AUTO\_ABORT

Enable/Disable the auto\_abort feature. Auto\_abort is disabled by default.

A.2.16 New ioctl USBTMC\_IOCTL\_API\_VERSION

Returns current API version of usbtmc driver.

This is to allow an instrument library to determine whether the driver API is compatible with the implementation.

The API may change in future versions. Therefore, the macro USBTMC\_API\_VERSION should be incremented when changing tmc.h with new flags, ioctls or when changing a significant behavior of the driver.

A.3 Test Functions

These ioctls are implemented in the intermediate github driver[[2]](#footnote-3) to simulate error conditions while testing. Because these ioctls are not part of the core driver functionality, they are not included in the USBTMC Linux kernel driver code.

A.3.1 USBTMC\_IOCTL\_SET\_OUT\_HALT

For testing: This ioctl sends a SET\_FEATURE(HALT) request to the OUT endpoint. The ioctl is useful for test purposes, to simulate a device that cannot receive any data due to an error condition.

A.3.2 USBTMC\_IOCTL\_SET\_IN\_HALT

For testing: This ioctl sends a SET\_FEATURE(HALT) request to the IN endpoint. The ioctl is useful for test purposes to simulate a device that cannot send any data due to an error condition.

A.3.3 USBTMC\_IOCTL\_ABORT\_BULK\_IN\_TAG

For testing: The ioctl tries to abort a BULK IN transfer with a given tag.

A.3.4 USBTMC\_IOCTL\_ABORT\_BULK\_OUT\_TAG

For testing: The ioctl tries to abort a BULK OUT transfer with a given tag.

1. For examples on the proper way to use this ioctl, refer to examples on the IVI git repository. [↑](#footnote-ref-2)
2. <https://github.com/GuidoKiener/linux-usbtmc> [↑](#footnote-ref-3)